Commands between server, cell phone and main controller

1. Register: /Register [email] [password]
   1. par[0] = email(username)
   2. par[1] = password
2. Login: /Login [username] [password]
   1. par[0] = username
   2. par[1] = password
3. Add Main Controller: /AddMC [username] [password] [MCID] [username]
   1. par[0] = username
   2. par[1] = password
   3. par[2] = Main Controller ID
   4. par[3] = username
4. Main Controller Connect: /MCConnect [MCID]
   1. par[0]= MCID
5. Control Appliance: /ControlAppliance [username] [password] [MCID] [Device Type] [Device ID] [cmd]
   1. par[0] = username
   2. par[1] = password
   3. par[2] = MCID
6. Get Light used data: /Chart [username] [password] [MCID] [Device]…
7. Get AC infor: /ChartInfo [username] [password] [MCID] [Device]…
8. Set time duration: /TimeSetting [username] [password] [starttime] [endtime]
9. Setting of energy saving: /EnergySaver [username] [password] [MCID]…
10. Setting of ideal temperature: /IdealTemperature [username] [password] [MCID]…
11. Notification to cell phone to tell if whether mission completed or not: /Notification [MCID] [message]
12. Change user password: /ChangePassword [username] [password] [newpassword]
    1. par[0] = username
    2. par[1] = password
    3. par[2] = newpassword